> # Configuring FCoE Using DCNM for SAN

> From Cisco NX-OS Release 5.2, FCoE is supported on MDS and Cisco Nexus 7000 switches. To enable or disable FCoE, Cisco MDS 9000 Family and Cisco Nexus 7000 switches uses feature set MIBs.

> ## Detailed Steps

> To configure FCoE on a switch, follow these steps:

> 1. In the Physical Attributes pane, choose Switches > FC Services > FCoE.

> You see the FCoE information pane.

> The Config tab displays the FCoE parameters for each Cisco Nexus 5000 Series, Cisco Nexus 7000 Series, and Cisco MDS 9000 Family switches. Use the VLAN-VSAN mapping tab to create mappings. Table 18-1 lists the FCoE parameters for a switch.

> For more information on configuring Cisco Nexus 5000 Series and Nexus 7000 Series switches, see the Cisco Nexus 5000 Series and Nexus 7000 Series Configuration Guides.

> Table 18-1 FCoE Parameters
> Parameter | Description
> --- | ---
> Feature Set | Enables or disables the FCoE feature set on Cisco MDS 9000 Family or Nexus 7000 Series switches.
> Control | Enables or disables FCoE on Cisco Nexus 5000 Series switches.
> Config | Displays the FCoE configuration information on the switch. For example, FC Map and FCF Priority.
> VLAN-VSAN Mapping | Displays the VSAN and VLAN IDs with their operational status.

> 2. Double-click the relevant FCoE parameter for a switch, and modify the value of the parameter.
> 3. In the Information pane toolbar, click the Apply Changes icon to save the changes.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.