> # Zoneset Members

> Field | Description
> --- | ---
> Zone | Default zone.
> Type | FCID.
> Switch Interface | Switch interface to which the zone member is connected to.
> Name | Zone member name.
> WWN | Zone member WWN.
> FcId | Zone member FC ID.
> Luns | Zone member LUN.
> Status | Not in Fabric: If zone member is not in the fabric. Not in VSAN: If zone member is not present in the VSAN. n/a: Cannot determine status. Empty: Member is present in fabric and correct VSAN and can communicate with other members of the zone.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.