> # Configuring FICON

> Fibre Connection (FICON) interface capabilities enhance the Cisco MDS 9000 Family by supporting both open systems and mainframe storage network environments. The control unit port (CUP) also is supported, which allows in-band management of the switch from FICON processors.

> Note Cisco Fabric Manager release 3.x does not support FICON management of Cisco MDS 9000 Family switches running SAN-OS release 2.(x).

> This chapter includes the following topics:

> - Information About FICON
> - Licensing Requirements for FICON
> - Guidelines and Limitations
> - Default Settings
> - Configuring FICON
> - Configuring FICON Ports
> - Verifying FICON Configuration
> - Field Descriptions for FICON
> - Additional References
> - Feature History for FICON

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.