> # FC-SP ESP Interfaces

> Field | Description
> --- | ---
> Interface | Name of the interface.
> ESP Mode | Specifies the ESP mode as one of the following: None-ESP is not running on the link. Gcm- Link needs to be encrypted and authenticated. Gmac-Link needs to be authenticated
> EgressSA | Specifies the egress security association to be used. Valid values are between 256 and 65536.
> IngressSA1 | Specifies the ingress security association to be used. Valid values are between 256 and 65536.
> IngressSA2 | Specifies the ingress security association to be used. Valid values are between 256 and 65536.
> EspFailureReason | Displays the reason of failure. “None” indicates that no error.

> #

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.