> # Configuring a LUN-Based Zone

> ## Detailed Steps

> To configure a LUN-based zone, follow these steps:

> 1. Choose Zone > Edit Local Full Zone Database.

> You see the Select VSAN dialog box.

> 2. Select a VSAN and click OK.

> You see the Edit Local Full Zone Database dialog box for the selected VSAN.

> 3. Click the zone where you want to add members and click the Insert icon.

> You see the Add Member to Zone dialog box.

> 1. Click either the WWN or FCID radio button from the Zone By options to create a LUN-based zone.
> 2. Check the LUN check box and click the browse button to configure LUNs.
> 3. Click Add to add this LUN-based zone.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.