> # Single SD Port to Monitor Traffic

> You do not need to use two SD ports to monitor bidirectional traffic on any interface. You can use one SD port and one FC analyzer port by monitoring traffic on the interface at the same SD port fc2/1.

> To use this setup, the analyzer should have the capability of distinguishing ingress and egress traffic for all captured frames.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.