> # FCIP Interfaces

> The FCIP interface is the local endpoint of the FCIP link and a VE port interface. All the FCIP and E port parameters are configured in context to the FCIP interface.

> The FCIP parameters consist of the following:

> - The FCIP profile determines which Gigabit Ethernet port initiates the FCIP links and defines the TCP connection behavior.
> - Peer information.
> - Number of TCP connections for the FCIP link.
> - E port parameters—trunking mode and trunk allowed VSAN list.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.