> # FCIP FICON Configuration

> Field | Description
> --- | ---
> Interface | This is a unique value that identifies the interface on this FCIP device to which this link pertains.
> VSAN List Admin | This is the list of VSANs (in the range 1 through 2047) for which FICON tape acceleration is configured. Only VSANs with a cficonVsanEntry of CISCO-FICON-MIB present can be configured for FICON tape acceleration.
> VSAN List Oper | This is the list of VSANs (in the range 1 through 2047) for which FICON tape acceleration is operationally ON.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.