> # Configuring the DHCHAP Mode

> To configure the DHCHAP mode for a particular interface, follow these steps:

> 1. Expand Switches, expand Interfaces, and then select FC Physical.

> You see the interface configuration in the Information pane.

> 2. Click the FC-SP tab.
> 3. Set the Mode drop-down menu to the DHCHAP authentication mode you want to configure for that interface.
> 4. Click the Apply Changes icon to save these DHCHAP port mode settings.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.