> # Configuring Load Balancing Using VRRP

> You must first configure VRRP on the Gigabit Ethernet interfaces on the switch that connect to the IP network before configuring VRRP for iSLB.

> ## Detailed Steps

> To configure VRRP load balancing using Device Manager, follow these steps:

> 1. Choose IP > iSCSI iSLB.

> You see the iSCSI iSLB dialog box.

> 2. Click the VRRP tab.
> 3. Click Create to configure VRRP load balancing for iSLB initiators.

> You see the Create iSCSI iSLB VRRP dialog box.

> 4. Set the Vrld to the VRRP group number.
> 5. Select either ipv4 or ipv6 and check the LoadBalance check box.
> 6. Click Create to enable load balancing.
> 7. If CFS is enabled, select commit from the CFS drop-down menu.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.