> # iSLB Initiator Targets

> You can configure initiator targets using the device alias or the pWWN. You can also optionally specify one or more of the following optional parameters:

> - Secondary pWWN
> - Secondary device alias
> - LUN mapping
> - IQN
> - VSAN identifier

> Note The VSAN identifier is optional if the target is online. If the target is not online, the VSAN identifier is required.

> In addition, you can disable auto-zoning.

> If you configure an IQN for an initiator target, then that name is used to identify the initiator target. Otherwise, a unique IQN is generated for the initiator target.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.