> # FICON Requirements

> The FICON feature has the following requirements:

> - You can implement FICON features in the following switches:
> - Any switch in the Cisco MDS 9500 Series
> - Any switch in the Cisco MDS 9200 Series (including the Cisco MDS 9222i Multiservice Modular Switch)
> - Cisco MDS 9134 Multilayer Fabric Switch
> - MDS 9000 Family 18/4-Port Multiservice Module
> - You need the MAINFRAME_PKG license to configure FICON parameters.
> - To extend your FICON configuration over a WAN link using FCIP, you need the appropriate SAN_EXTN_OVER_IP license for the module you are using. For more information, refer to the Cisco NX-OS Family Licensing Guide.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.