> # Trunking F Ports

> Trunking F ports allows interconnected ports to transmit and receive tagged frames in more than one VSAN, over the same physical link.

> Link Number | Link Description
> --- | ---
> 1a and 1b | F port trunk with N port.1
> 2 | F port trunk with NP port.
> 3 | F PortChannnel with NP port.
> 4 | Trunked F PortChannel with NP port.
> 5 | Trunking NP port with third-party core switch F port.1

> 1These features are not supported currently.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.