> # Configuring Interface Modes

> ## Detailed Steps

> To configure the interface mode using DCNM-SAN, follow these steps:

> 1. Expand Switches > FC Interfaces > Physical.

> You see the interface configuration in the Information pane.

> 2. Click the General tab.
> 3. Click Mode Admin. Set the desired interface mode from the Admin drop-down menu.
> 4. (Optional) Set other configuration parameters using the other tabs.
> 5. Click Apply Changes icon.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.