> # Ethernet Interface Monitor TCP

> Field | Description
> --- | ---
> Opens | The number of times connections have been opened.
> Accepts | The number of times connections have been accepted.
> Failed | The number of times connections have failed.
> RxResets | The number of times connections have been reset.
> Est | The number of connections that have been established.
> RxSegs | The total number of segments received on established connections, including those received in error.
> TxSegs | The total number of segments sent, except for those containing retransmitted bytes.
> ReTxSegs | The total number of segments retransmitted.
> BadSegs | The total number of segments received in error (e.g., bad checksums).
> TxSegResets | The number of segments sent containing the "reset" flag.
> SplitSeg | The number of segments sent which were less than the minimum.
> DupACKs | The number of duplicate ACKs received.
> RxBytes | The number of header and data bytes received.
> TxBytes | The number of header and data bytes sent.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.