> # Port Guard

> Field | Description
> --- | ---
> Interface | Name of the interface
> Enable | Specifies whether an interface can be stopped from changing between up and down states or allowed to change states continuously.
> Duration (sec) | Specifies the time duration in which a port is allowed to change states.
> Number of Flaps | Specifies the number of times the port can flap in the time specified in the Duration.
> Oper | Operational state of the interface.

> #

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.