> # Enabling SCSI Flow Statistics

> ## Detailed Steps

> To enable SCSI flow statistics monitoring using DCNM-SAN, follow these steps:

> 1. Expand End Devices and then select SSM Features in the Physical Attributes pane.

> You see the FCWA tab in the Information pane.

> 2. Click Create Row in the Information pane to create a SCSI flow or click a row in the FCWA table to modify an existing SCSI flow.

> You see the FC Write Acceleration dialog box.

> 3. Select the initiator and target WWNs and VSAN IDs and check the Enable Statistics check box to enable SCSI flow statistics on this SCSI flow.
> 4. (Optional) Enable Fibre Channel Write Acceleration on this SCSI flow at this time by checking the WriteAcc check box.
> 5. Click Create to create this SCSI flow.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.