> # Initiator Specific Target

> Field | Description
> --- | ---
> Name | A globally unique identifier for the node.
> Port WWN(s) Primary | The Fibre Channel target's port addresses associated with this iSCSI initiator-specific target.
> Port WWN(s) Secondary | The Fibre Channel target's port addresses associated with this iSCSI initiator-specific target.
> LUN Map (Hex) iSCSI | The Fibre Channel target's port addresses associated with this iSCSI initiator-specific target.
> LUN Map (Hex) FC Primary | The Fibre Channel target's port addresses associated with this iSCSI initiator-specific target.
> LUN Map (Hex) FC Secondary | The Fibre Channel target's port addresses associated with this iSCSI initiator-specific target.
> No AutoZone Creation | Indicates if a Fibre Channel zone is automatically created for this iSCSI initiator-target and the iSCSI initiator. If true the zone is not automatically created. If false (default) the zone is automatically created.
> Trespass Mode | The trespass mode for this node. If true the Fibre Channel node instance presents all LUN I/O requests to the secondary port (fcSecondaryAddress) if the primary port (fcAddress) is down.
> Revert to Primary Port | The revert to primary mode for this node. If true the Fibre Channel node instance presents all LUN I/O requests to the primary port fcAddress) when the primary port comes back online.
> Primary PWWN VSAN | Indicates the VSAN into which the auto zone is placed for this initiator target. If this object is not set then the VSAN is determined by querying the name server.
> Secondary PWWN VSAN | Indicates the VSAN into which the auto zone is placed for this initiator target. If this object is not set then the VSAN is determined by querying the name server.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.