> # IVR Zoneset Active Zones Attributes

> Field | Description
> --- | ---
> Zone | Active IVR zone name.
> QoS | True if QoS enabled, otherwise false.
> QoS Priority | QoS priority value (Low, Medium, or High).
> Broadcast | Specifies if broadcast zoning is enabled on this default zone on this VSAN. If true, then it is enabled. If false, then it is disabled.

> Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.