> # Configuring SFTP

> You can configure the SFTP credentials for a switch.

> 1. From the menu bar, choose Admin > General > SFTP/TFTP Credentials.
>    You see the SFTP/TFTP credentials page.
> 2. In the Server Type field, use the radio button to select SFTP.
> 3. Enter the SFTP Username and SFTP Password.
> 4. Enter the Root Directory path.
> 5. From the Verification Switch drop-down, select the switch.
> 6. Click Apply to apply the configuration.
> 7. Click Apply and Verify to apply and verify the configuration.
> 8. Click Clear SSH Hosts to clear SSH hosts for all switches or selected switches. If there is a failure in any of the switches, an error message is displayed. Go to Admin>Logs>Web Report to view the number of successful and unsuccessful switches.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.