> # Fibre Channel PortChannels

> The following characteristics set Fibre Channel PortChannel solutions apart from other solutions:

> - The entire bundle is one logical (E)ISL link.
> - All FCIP links in the PortChannel should be across the same two switches.
> - The Fibre Channel traffic is load balanced across the FCIP links in the PortChannel.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.