> # Configuring the DHCHAP Timeout Value

> To configure the DHCHAP timeout value, follow these steps:

> 1. Expand Switches > Security, and then select FC-SP.

> You see the FC-SP configuration in the Information pane.

> 2. Click the General/Password tab.

> You see the DHCHAP general settings mode for each switch.

> 3. Change the DHCHAP timeout value for each switch in the fabric.
> 4. Click the Apply Changes icon to save the updated information.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.