## Creating an Edge Router

1. From the menu bar, select Config > Border Leaf Device Pairing.

2. Click Add. Select Edge Router.

3. To configure the Edge Router:

a. Use the radio button to select Configure an Edge Router.

Note The Configure an Edge Router option will be selected by default.

b. Select Notify Edge Router when relevant partitions are changed to notify the Edge Router.

c. Select the Device Name from the drop-down list to identify an Edge Router.

d. Specify the IP Address for the Edge Router.

e. Specify the Maximum Number of Partitions required for the Edge Router.

4. To configure a Hub-PE:

a. Use the radio button to select Configure a Hub-PE.

b. Select Notify Edge Router when relevant partitions are changed to notify the Edge Router.

c. Select the Device Name from the drop-down list to identify an Edge Router.

d. Specify the IP Address for the Edge Router.

e. Specify the Maximum Number of Partitions required for the Edge Router.

f. Define the Profile Parameters.

– asn—specifies the autonomous system (AS) number for the Hub-PE

– vrfSegmentId—specifies the vrf segment ID.

– rsvdGlobalAsn—specifies the reserved global autonomous system number.

– dciId—specifies the Edge Router ID for the Hub-PE

– vrfName—Specifies the vrf name

Note Note: The value for vrfName must be of the format 'organizationName:partitionName'.

5. Click OK to save the configuration.