> # Bandwidth Reservation: 24-Port 48-Gbps Fibre Channel Module

> RateMode Configuration Macro | Description
> --- | ---
> Dedicated 8 Gbps on the first port of each group and the remaining ports 8 Gbps shared | Allocates a rate mode of 8Gbps on the first port of each group and the remaining ports share 8 Gbps depending on the operational speed of the ports.
> Shared Auto on all ports (initial and default settings) | Allocates a rate mode of 8 Gbps on all the available ports. This is the default setting.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.