> # Configuring iSCSI

> This section describes how to configure iSCSI on the Cisco MDS 9000 Family switches.

> This section includes the following sections:

> - Enabling iSCSI
> - Creating iSCSI Interfaces
> - Using the iSCSI Wizard
> - Enabling Dynamic Mapping
> - Creating Static Mapping
> - Advertising Static iSCSI Targets
> - Specifying the Initiator Identification
> - Configuring the iSCSI Initiator Idle Timeout
> - Configuring Static Mapping
> - Making the Dynamic iSCSI Initiator WWN Mapping Static
> - Checking for WWN Conflicts
> - Configuring the Proxy Initiator
> - Configuring VSAN Membership for iSCSI Hosts
> - Configuring Default Port VSAN for iSCSI Interfaces
> - Adding iSCSI Initiator to the Zone Database
> - Configuring Access Control in iSCSI
> - Configuring AAA Authentication for an iSCSI User
> - Configuring Authentication Mechanism
> - Configuring iSLB Using Device Manager
> - Assigning VSAN Membership for iSLB Initiators
> - Configuring and Activating Zones for iSLB Initiators and Initiator Targets
> - Restricting iSLB Initiator Authentication

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.