> # DPVM Actions

> Field | Description
> --- | ---
> Action | Helps in activating the set of bindings.
> Result | Indicates the outcome of the activation.
> Status | Indicates the state of activation. If true, then activation has been attempted as the most recent operation. If false, then an activation has not been attempted as the most recent operation.
> CopyActive to Config | When set to copy(1), results in the active (enforced) binding database to be copied on to the configuration binding database. The learned entries are also copied.
> Auto Learn Enable | Helps to learn the configuration of devices logged into the local device on all its ports and the VSANs to which they are associated.
> Auto Learn Clear | Assists in clearing the auto-learnt entries.
> Clear WWN | Represents the Port WWN (pWWN) to be used for clearing its corresponding auto-learnt entry.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.