> # NP Ports

> An NP port is a port on a device that is in NPV mode and connected to the core switch via an F port. NP ports function like N ports except that in addition to providing N port operations, they also function as proxies for multiple, physical N ports.

> Note A Cisco Nexus 5000 Series switch in NPV mode that runs Cisco NX-OS Release 4.2(1) or later releases supports trunking F port mode on NP ports. You can enable either, or both, VSAN trunking and an F port on an NP port.

> For more details about NP ports and NPV, see "Configuring N Port Virtualization."

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.