> # FC Interfaces Capability

> Field | Description
> --- | ---
> FC-PH Vers Low | The lowest version of FC-PH that the FC-Port is capable of supporting.
> FC-PH Vers High | The highest version of FC-PH that the FC-Port is capable of supporting.
> RxDataSize Min | The minimum size in bytes of the Data Field in a frame that the FC-Port is capable of receiving from its attached FC-port.
> RxDataSize Max | The maximum size in bytes of the Data Field in a frame that the FC-Port is capable of receiving from its attached FC-port.
> HoldTime Min | The minimum holding time (in microseconds) that the FC-Port is capable of supporting.
> HoldTime Max | The maximum holding time (in microseconds) that the FC-Port is capable of supporting.
> CoS | The Bit mask indicating the set of Classes of Service that the FC-Port is capable of supporting.
> ServiceStateCapable | Indicates whether this interface is capable of handling service state change.
> PortRateMode Capable | Indicates whether this interface is capable of being configured as dedicated or shared port rate modes.
> AdminRxBbCreditExtended Capable | If true, it is capable of changing the extended buffer-to-buffer credits on the interface. The user can configure the object fcIfAdminRxBbCreditExtended on this interface
> Class2Seq Deliv | The flag indicating whether or not the FC-Port is capable of supporting Class 2 Sequential Delivery.
> Class3Seq Deliv | The flag indicating whether or not the FC-Port is capable of supporting Class 3 Sequential Delivery.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.