> # Suspending a FICON VSAN

> ## Detailed Steps

> To suspend a FICON VSAN, follow these steps:

> 1. Click All VSANs.

> You see all the VSANs listed in the Information pane.

> 2. Select the VSAN that you want to suspend.
> 3. Set the Admin drop-down menu for a VSAN to suspended.
> 4. Click the Apply Changes icon to save these changes.

> Note This command can be issued by the host if the host is allowed to do so (see the "Allowing the Host to Move the Switch Offline" topic).

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.