> # Using the iSCSI Wizard

> ## Detailed Steps

> To use the iSCSI wizard in Cisco DCNM-SAN, follow these steps:

> 1. Click the iSCSI Setup Wizard icon.

> You see the iSCSI Wizard Configure Initiator dialog box.

> 2. Select an existing iSCSI initiator or add the iSCSI node name or IP address for a new iSCSI initiator.
> 3. Select the switch for this iSCSI initiator if you are adding a new iSCSI initiator and click Next.

> You see the iSCSI Wizard Select Targets dialog box.

> 4. Select the VSAN and targets to associate with this iSCSI initiator and click Next.

> Note The iSCSI wizard turns on the Dynamic Import FC Targets feature.

> You see the iSCSI Wizard Select Zone dialog box.

> 5. Set the zone name for this new iSCSI zone and check the ReadOnly check box if needed.
> 6. Click Finish to create this iSCSI initiator.

> If created, the target VSAN is added to the iSCSI host VSAN list.

> Note iSCSI wizard automatically turns on the Dynamic FC target import.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.