> # Configuring IPS Core Dumps

> ## Detailed Steps

> To configure the Gigabit Ethernet interface, follow these steps:

> 1. From Cisco DCNM-SAN, choose Switches > Interfaces > Gigabit Ethernet in the Physical Attributes pane. You see the Gigabit Ethernet configuration in the Information pane.

> From Device Manager, right-click the Gigabit Ethernet port that you want to configure and choose Configure.... You see the Gigabit Ethernet configuration dialog box.

> 2. Click the General tab in Cisco DCNM-SAN, or click the GigE tab in Device Manager to display the general configuration options for the interface.
> 3. Set the description and MTU value for the interface. The valid value for the MTU field can be a number in the range from 576 to 9000.
> 4. Set Admin up or down and check the CDP check box if you want this interface to participate in CDP.
> 5. Set IpAddress/Mask with the IP address and subnet mask for this interface.
> 6. From Cisco DCNM-SAN, click the Apply Changes icon to save these changes, or click the Undo Changes icon to discard changes.

> From Device Manager, click Apply to save these changes, or click Close to discard changes and close the Gigabit Ethernet configuration dialog box.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.