> # Ethernet Interfaces VLAN

> Field | Description
> --- | ---
> Switch | Name of the switch.
> Interface | Name of the interface.
> VLAN mode | The mode in which this VLAN is configured. Static—A port with static VLAN membership directly assigned to a single VLAN. Dynamic—A port with dynamic VLAN membership assigned to a single VLAN based on the content of packets received on the port via VQP queries to VMPS. multiVLAN—A port with multiple VLAN memberships that are directly assigned to one or more VLANs.
> VLAN list | The list of VLANs which are allowed on the switch.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.