> # FC-SP Interfaces

> Field | Description
> --- | ---
> Mode | The FC-SP mode on this interface. If autoPassive, a port would not initiate any FC-SP authentication exchange; but would always take part in FC-SP authentication exchange initiated by the other side. If autoActive, a port would always try to initiate FC-SP authentication exchange after ESC. If other side does not support FC-SP authentication, port will still be brought up. If on, port would always try to initiate FC-SP authentication exchange and authentication is done before the port becomes up. If other side does not support FC-SP authentication, port will not be brought up. If off, port would never initiate FC-SP authentication exchange and send reject to any FC-SP authentication message started from other end. If this is not 'off', then port has to support at least one FC-SP authentication protocol.
> Reauthenticate Interval (hr) | The time (in hours) for which a port has to wait before trying to re-authenticate the other end.
> Reauthenticate Start | Re-authenticate the other end, if this is set to enable.
> Auth Successes | The number of times the FC-SP authentication succeeded on this interface.
> Auth Fails | The number of times the FC-SP authentication failed on this interface.
> Auth Bypasses | The number of times the FC-SP authentication was bypassed on this interface.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.