> # AAA LDAP Servers

> Field | Description
> --- | ---
> IP Address Type | The IP address type (IPv4, IPv6, or DNS).
> Name or IP Address | The name or IP address of the AAA server.
> AuthPort | The Authentication port of the AAA server.
> TimeOut(s) | The time in seconds between retransmissions to the AAA server.This value overrides value set in the timeout set in the Features tab for this server. If this value is zero, then the value set in the Features tab will be used.
> Retransmits | The additional number of times the AAA server should be tried by the AAA client before giving up on the server. This value overrides value set in the Features tab. If this value is zero, then the value set in the Features tab will be used.
> Idle Time (m) | The time interval in minutes, at which the system periodically tests the AAA Server by sending test packets to the server. The default value of 0 means that the AAA server is not tested periodically.
> TestUser | The user name to be used in the test packets sent to the AAA Server, to test if the server responds to the requests.
> TestPassword | The password to be used in test packets sent to the AAA Server to test if the server responds to the requests.
> RootDN | The root name that is used for authenticating access to LDAP server database.
> RootDNPasswordEncrType | Type of encryption that is used for the RootDNPassword password.
> RootDNPassword | The RootDN password to use if you want to perform root binding. Anonymous bind will be performed if you do not enter a RoodDN password.
> SSL Mode | Specifies whether the TLS tunnel needs be setup or not, before binding with the LDAP server.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.