> # Default Settings

> Table 28-3 lists the default settings for the features included in this chapter.

> Table 28-3 Default Settings for Advanced Features
> Parameters | Default
> --- | ---
> CIM server | Disabled
> CIM server security protocol | HTTP
> D_S_TOV | 5,000 milliseconds.
> E_D_TOV | 2,000 milliseconds.
> R_A_TOV | 10,000 milliseconds.
> Timeout period to invoke fctrace | 5 seconds.
> Number of frame sent by the fcping feature | 5 frames.
> Remote capture connection protocol | TCP.
> Remote capture connection mode | Passive.
> Local capture frame limit s | 10 frames.
> FC ID allocation mode | Auto mode.
> Loop monitoring | Disabled.
> D_S_TOV | 5,000 msec
> E_D_TOV | 2,000 msec
> R_A_TOV | 10,000 msec
> Interop mode | Disabled

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.