> # Call Home Destination Profiles

> A destination profile contains the required delivery information for an alert notification. Destination profiles are typically configured by the network administrator.

> Using alert groups you can select the set of Call Home alerts to be received by a destination profile (predefined or user defined). Alert groups are predefined subsets of Call Home alerts supported in all switches in the Cisco MDS 9000 Family and the Cisco Nexus 5000 Series. Different types of Call Home alerts are grouped into different alert groups depending on their type. You can associate one or more alert groups to each profile as required by your network.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.