> # Fibre Channel Zoning-Based Access Control

> Cisco SAN-OS Release 3.x and NX-OS Release 4.1(1b) VSAN and zoning concepts have been extended to cover both Fibre Channel devices and iSCSI devices. Zoning is the standard access control mechanism for Fibre Channel devices, which is applied within the context of a VSAN. Fibre Channel zoning has been extended to support iSCSI devices, and this extension has the advantage of having a uniform, flexible access control mechanism across the whole SAN.

> Common mechanisms for identifying members of a Fibre Channel zone are the following:

> - Fibre Channel device pWWN.
> - Interface and switch WWN. Device connecting via that interface is within the zone.

> See the Fabric Configuration Guide,Cisco DCNM for SAN for details on Fibre Channel zoning.

> In the case of iSCSI, multiple iSCSI devices may be connected behind an iSCSI interface. Interface-based zoning may not be useful because all the iSCSI devices behind the interface will automatically be within the same zone.

> In transparent initiator mode (where one Fibre Channel virtual N port is created for each iSCSI host as described in the "Transparent Initiator Mode" topic), if an iSCSI host has static WWN mapping then the standard Fibre Channel device pWWN-based zoning membership mechanism can be used.

> Zoning membership mechanism has been enhanced to add iSCSI devices to zones based on the following:

> - IPv4 address/subnet mask
> - IPv6 address/prefix length
> - iSCSI qualified name (IQN)
> - Symbolic-node-name (IQN)

> For iSCSI hosts that do not have a static WWN mapping, the feature allows the IP address or iSCSI node name to be specified as zone members. Note that iSCSI hosts that have static WWN mapping can also use these features. IP address based zone membership allows multiple devices to be specified in one command by providing the subnet mask.

> Note In proxy initiator mode, all iSCSI devices connecting to an IPS port gain access to the Fibre Channel fabric through a single virtual Fibre Channel N port. Zoning based on the iSCSI node name or IP address will not have any effect. If zoning based on pWWN is used, then all iSCSI devices connecting to that IPS port will be put in the same zone. To implement individual initiator access control in proxy initiator mode, configure an iSCSI ACL on the virtual target (see the "iSCSI-Based Access Control" topic).

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.