> # Virtual FC Ethernet

> Field | Description
> --- | ---
> Switch | Name of the switch hosting this interface.
> Interface | Displays the name of the vFC interface and its association with other interfaces.
> Description | Text description of the interface as specified by a network manager.
> Status Admin | The desired state of the interface.
> Status Oper | The current operational state of the interface.
> Speed Oper | Operational speed of the interface
> LastChange | When the interface entered its current operational state. If the current state was entered prior to the last re-initialization of the local network management subsystem, then this value is N/A.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.