> # Zone Implementation

> All switches in the Cisco MDS 9000 Family automatically support the following basic zone features (no additional configuration is required):

> - Zones are contained in a VSAN.
> - Hard zoning cannot be disabled.
> - Name server queries are soft-zoned.
> - Only active zone sets are distributed.
> - Unzoned devices cannot access each other.
> - A zone or zone set with the same name can exist in each VSAN.
> - Each VSAN has a full database and an active database.
> - Active zone sets cannot be changed, without activating a full zone database.
> - Active zone sets are preserved across switch reboots.
> - Changes to the full database must be explicitly saved.
> - Zone reactivation (a zone set is active and you activate another zone set) does not disrupt existing traffic.

> If required, you can additionally configure the following zone features:

> - Propagate full zone sets to all switches on a per VSAN basis.
> - Change the default policy for unzoned members.
> - Interoperate with other vendors by configuring a VSAN in the interop mode. You can also configure one VSAN in the interop mode and another VSAN in the basic mode in the same switch without disrupting each other.
> - Bring E ports out of isolation.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.