> # Configuring TL Ports

> Private loops require setting the interface mode to TL.

> ## Detailed Steps

> To configure the TL interface mode using DCNM-SAN, follow these steps:

> 1. Expand Switches > FC Interfaces > Physical. You see the interface configuration in the Information pane.
> 2. Click the General tab and click Mode Admin.
> 3. Set the Mode Admin drop-down menu to the required status.
> 4. (Optional) Set other configuration parameters using the other tabs.
> 5. Click Apply Changes.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.