> # iSNS Cloud Discovery

> Field | Description
> --- | ---
> AutoDiscovery | Whether automatic cloud discovery is turned on or off.
> DiscoveryDelay | Time duration between successive IP cloud discovery runs.
> Discovery | The IP network discovery command to be executed. all- Run IP network discovery for all the gigabit Ethernet interfaces in the fabric. noOp (default)- No operation is performed.
> CommandStatus | The status of the license install / uninstall / update operation. success— Discovery operation completed successfully. nProgress— Discovery operation is in progress. none— No discovery operation is performed. NoIpNetworkNameSpecified— IP Cloud name not specified. invalidNetworkName— IP Cloud is not configured. NoIPSPortNameSpecified— Gigabit Ethernet port if index not specified. invalidIPSPortName— Invalid Gigabit Ethernet port interface. generalISNSFailure— General ISNS server failure.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.