> # Enabling Cisco TrustSec FC Link Encryption

> By default, the FC-SP feature and the Cisco TrustSec FC Link Encryption feature are disabled in all switches in the Cisco MDS 9000 Family.

> You must explicitly enable the FC-SP feature to access the configuration and verification commands for fabric authentication and encryption. When you disable this feature, all related configurations are automatically discarded.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.