<!DOCTYPE html PUBLIC "-//W3C//DTD XHTML 1.0 Transitional//EN" "http://www.w3.org/TR/xhtml1/DTD/xhtml1-transitional.dtd">

<!-- saved from url=(0014)about:internet -->
<html xmlns="http://www.w3.org/1999/xhtml" xml:lang="en" lang="en">
  <head>
    <meta http-equiv="Content-Type" content="text/html; charset=UTF-8" />
    <meta http-equiv="Content-Style-Type" content="text/css" />
    <meta name="GENERATOR" content="Quadralay WebWorks AutoMap 2003 Platinum Edition Client for FrameMaker 8.6.6597.0" />
    <meta name="TEMPLATEBASE" content="emwebh8-1-17" />
    <meta name="LASTUPDATED" content="08/01/13 14:48:02" />
    <title>Assigning a Peer IP Address  </title>
    <!-- Copyright 2010-2013, Cisco Systems, Inc. All rights reserved. -->

    <link rel="StyleSheet" href="document.css" type="text/css" />
    <link rel="StyleSheet" href="catalog.css" type="text/css" />


<script> 
    var is_chrome = navigator.userAgent.toLowerCase().indexOf('chrome') > -1; 
   
    if(is_chrome){document.domain=document.domain}
   </script>
    <script type="text/javascript" language="JavaScript1.2" src="expand.js"></script>
    <script type="text/javascript" language="JavaScript1.2" src="page.js"></script>

    <script type="text/javascript" language="JavaScript1.2">
     <!--
      function  WWNoOp() {}
      function  WWNoValue() { return ""; }

      var  VarDropDown;

      if (typeof(HTMLHelp_Object) != "undefined")
      {
        VarDropDown = new WWDropDown_Object();
      }
      else
      {
        VarDropDown = new Object();
        VarDropDown.fAnchorOpen  = WWNoOp;
        VarDropDown.fAnchorClose = WWNoOp;
        VarDropDown.fDIVOpen  = WWNoOp;
        VarDropDown.fDIVClose = WWNoOp;
      }
     // -->
    </script>

  
<SCRIPT language="javascript">
<!--
  self.document.write("<link href='"+top.relPath+"shared/style.css' rel='stylesheet' type='text/css'>");
  myid=1871;
  self.document.write("<script type='text/javascript' language='JavaScript' src='"+top.relPath+"shared/con_utils.js'></scr"+"ipt>");
//-->
</SCRIPT>
</head>

  <body onload="highlightSearchTerms();" bgcolor="#ffffff">

    
    <blockquote>
    <a name="top"></a>

    
    


<a name="wp1075750"> </a><h1 class="pTitle">
Assigning a Peer IP Address 

</h1>
<a name="wp1075752"> </a><p class="pBody">
The basic FCIP configuration uses the peer’s IP address to configure the peer information. You can also 
specify the peer’s port number to configure the peer information. If you do not specify a port, the default 
3225 port number is used to establish connection. You can specify an IPv4 address or an IPv6 address.

</p>
<a name="wp1097998"> </a><h2 class="pHeading2">
Detailed Steps
</h2>
<a name="wp1152723"> </a><p class="pBody">
To assign the peer information based on the IPv4 address and port number, follow these steps:

</p>
<div class="pSmartList1"><ol type="1" class="pSmartList1">
<a name="wp1152724"> </a><li class="pSmartList1">Expand <span style="font-weight: bold">ISLs</span> and select<span style="font-weight: bold"> FCIP</span> in the Physical Attributes pane. 
</li>
<a name="wp1152725"> </a><p class="pListBodyLevel1">
You see the FCIP profiles and links in the Information pane.

</p>
<a name="wp1152726"> </a><p class="pListBodyLevel1">
From Device Manager, choose <span style="font-weight: bold">IP &gt; FCIP</span>.

</p>
<a name="wp1152727"> </a><p class="pListBodyLevel1">
You see the FCIP dialog box.

</p>
<a name="wp1152728"> </a><li class="pSmartList1">Click the <span style="font-weight: bold">Tunnels</span> tab. You see the FCIP link information.
</li>
<a name="wp1152729"> </a><li class="pSmartList1">Click the <span style="font-weight: bold">Create Row</span> icon in DCNM-SAN or the <span style="font-weight: bold">Create</span> button in Device Manager. 
</li>
<a name="wp1152730"> </a><p class="pListBodyLevel1">
You see the FCIP Tunnels dialog box.

</p>
<a name="wp1152731"> </a><li class="pSmartList1">Set the ProfileID and TunnelID fields.
</li>
<a name="wp1152732"> </a><li class="pSmartList1">Set the RemoteIPAddress and RemoteTCPPort fields for the peer IP address you are configuring.
</li>
<a name="wp1152733"> </a><li class="pSmartList1">Check the <span style="font-weight: bold">PassiveMode</span> check box if you do not want this end of the link to initiate a TCP connection.
</li>
<a name="wp1152734"> </a><li class="pSmartList1">(Optional) Set the <span style="font-weight: bold">NumTCPC</span>on field to the number of TCP connections from this FCIP link.
</li>
<a name="wp1152735"> </a><li class="pSmartList1">(Optional) Check the <span style="font-weight: bold">Enable</span> check box in the Time Stamp section and set the Tolerance field.
</li>
<a name="wp1152736"> </a><li class="pSmartList1">(Optional) Set the other fields in this dialog box and click <span style="font-weight: bold">Create</span> to create this FCIP link.
</li>
</ol></div>
<a name="wp1152782"> </a><p class="pBody">
To assign the peer information based on the IPv6 address and port number, follow these steps:

</p>
<div class="pSmartList1"><ol type="1" class="pSmartList1">
<a name="wp1152783"> </a><li class="pSmartList1">From DCNM-SAN, choose <span style="font-weight: bold">ISLs &gt; FCIP</span> from the Physical Attributes pane. 
</li>
<a name="wp1152784"> </a><p class="pListBodyLevel1">
You see the FCIP profiles and links in the Information pane.

</p>
<a name="wp1152785"> </a><p class="pListBodyLevel1">
From Device Manager, choose <span style="font-weight: bold">IP &gt; FCIP</span>. You see the FCIP dialog box.

</p>
<a name="wp1152786"> </a><li class="pSmartList1">Click the <span style="font-weight: bold">Tunnels</span> tab. You see the FCIP link information.
</li>
<a name="wp1152787"> </a><li class="pSmartList1">Click the <span style="font-weight: bold">Create Row</span> icon in DCNM- SAN or the <span style="font-weight: bold">Create</span> button in Device Manager. 
</li>
<a name="wp1152788"> </a><p class="pListBodyLevel1">
You see the FCIP Tunnels dialog box.

</p>
<a name="wp1152789"> </a><li class="pSmartList1">Set the ProfileID and TunnelID fields.
</li>
<a name="wp1152790"> </a><li class="pSmartList1">Set the RemoteIPAddress and RemoteTCPPort fields for the peer IP address you are configuring.
</li>
<a name="wp1152791"> </a><li class="pSmartList1">Check the <span style="font-weight: bold">PassiveMode</span> check box if you do not want this end of the link to initiate a TCP connection.
</li>
<a name="wp1152792"> </a><li class="pSmartList1">(Optional) Set the <span style="font-weight: bold">NumTCPCon</span> field to the number of TCP connections from this FCIP link.
</li>
<a name="wp1152793"> </a><li class="pSmartList1">(Optional) Check the <span style="font-weight: bold">Enable</span> check box in the Time Stamp section and set the Tolerance field.
</li>
<a name="wp1152794"> </a><li class="pSmartList1">(Optional) Set the other fields in this dialog box and click <span style="font-weight: bold">Create</span> to create this FCIP link.
</li>
</ol></div>
<hr /><br><p class="pBody">Copyright 2010-2013, Cisco Systems, Inc. All rights reserved.</p> 

    </blockquote>

  </body>
</html>
