> # Configuring the Default Zone Access Permission

> ## Detailed Steps

> To permit or deny traffic to members in the default zone, follow these steps:

> 1. Expand a VSAN and then select Default Zone in the DCNM-SAN Logical Domains pane.
> 2. Click the Policies tab in the Information pane.

> You see the zone policies information in the Information pane.

> The active zone set is shown in italic type. After you make changes to the active zone set and before you activate the changes, the zone set is shown in boldface italic type.

> 3. In the Default Zone Behaviour field, choose either permit or deny from the drop-down menu.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.