> # Configuring the MTU Frame Size

> You can configure the interfaces on a switch to transfer large (or jumbo) frames on a port. The default IP maximum transmission unit (MTU) frame size is 1500 bytes for all Ethernet ports. By configuring jumbo frames on a port, the MTU size can be increased up to 9000 bytes.

> Note The minimum MTU size is 576 bytes.

> Tip MTU changes are disruptive, all FCIP links and iSCSI sessions flap when the software detects a change in the MTU size.

> ## Detailed Steps

> To configure the MTU frame size, follow these steps:

> 1. Expand Switches > Interfaces > Ethernet > IPS.

> You see the Gigabit Ethernet Configuration in the Information pane.

> 2. In the General tab, in the Mtu column, you can enter a new value to configure the MTU Frame Size for a specific switch. For example 3000 bytes. The default is 1500 bytes.
> 3. Click Apply Changes.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.