> # Rejecting Incoming RCFs

> ## Detailed Steps

> To reject incoming RCF request frames, follow these steps:

> 1. Expand Switches > FC Interfaces and then select Physical in the Physical Attributes pane.

> You see the Fibre Channel configuration in the Information pane.

> 2. Click the Domain Mgr tab.

> 3. Check the RcfReject check box for each interface that you want to reject RCF request frames on.
> 4. Click the Apply Changes icon to save these changes.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.