> # NASB Target

> Field | Description
> --- | ---
> Module, VSAN Id, Processor Id | The unique ID number associated with the TPC target. This ID number is unique within the VSAN in which the TPC target is configured.
> Virtual Target Node WWN | The TPC target's node world wide name.
> Virtual Target Port WWN | The TPC target's port world wide name.
> State | The current state of the TPC target.
> XCOPY Num | The total number of xcopy commands processed by the TPC target since the module on which this target has been configured has been online.
> XCOPY MinData (KB) | The smallest amount of data in kilobytes transferred by the TPC target in a single xcopy command since the module on which this target has been configured has been online.
> XCOPY MaxData (KB) | The largest amount of data in kilobytes transferred by the TPC target in a single xcopy command since the module on which this target has been configured has been online.
> XCOPY Avgthruput (KBps) | The average kilobytes per second throughput of the TPC target in processing the xcopy commands.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.