Editing an existing DHCP Scope

Note Once the DCNM is accessed for the first time, you must edit the default scope named 'enhanced_fab_mgmt" and add free IP address ranges.

1. From the menu bar, select Config>Power-On Auto Provisioning (POAP)>DHCP Scope.

2. Use the checkbox to select the DHCP scope.

3. Click Edit scope icon.

4. In the Edit DHCP Scope window, edit the DHCP scopes.

5. Click Apply to save the changes.