> # About Fibre Channel Routes

> Each port implements forwarding logic, which forwards frames based on its FC ID. Using the FC ID for the specified interface and domain, you can configure the specified route (for example FC ID 111211 and domain ID 3) in the switch with domain ID 1.

> Note Other than in VSANs, runtime checks are not performed on configured and suspended static routes.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.