> # QoS Match Statements

> Field | Description
> --- | ---
> SrcAddr | An FC address that needs to be matched with the source address in a FC frame.
> DstAddr | An FC address that needs to be matched with the destination address in a FC frame.
> Interface | An FC interface on the local device on which a frame should arrive in order to be classified by this filter. A value of zero indicates that no interface is configured.
> WildCard | Specifies whether the wild-card option has been set. If true, then the wild-card option is set and all the FC traffic will be considered to match the corresponding multi-field classifier. If false, then the wild-card option is not set.

> Copyright 2010-2015, Cisco Systems, Inc. All rights reserved.